Event xx:yy

I/O 1 – output “point A”

I/O 2 – servo “point A”

I/O 3 – output “relay A”

I/O 1 – input “switch”

Node C

“LED Panel”

Node B

Consumer A

Node A

“switches”

Event xx:yy

“switch 1”

Event xx:yy

Event xx:yy